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	Work Process Schedule
	
	OJT HRS

	Plan reading and interpretation

Reading shop drawings

Symbols and abbreviations

Familiarization with NFPA 13, NFPA 14, NFPA 20, and NFPA 24

	
	800

	Care of tools, materials, and equipment

Identifying materials, grades and types of pipe, fittings, valves, hose and equipment, and fire sprinklers

Use and operation of trade tools

Maintaining and servicing of tools and equipment

Safety meetings

	
	800

	Preparation of tools, materials, and equipment

Selection of pipe, fittings, hangers, and devices for rough and finish work

Loading of required materials and equipment

Unloading of materials and equipment at job site using safety

Set up and use of rigging, scaffolding and mechanical lifts, and platforms

Safety meetings

	
	650

	Pipe cutting, threading, reaming, and welding

Use of hand cutters

Use of dies and reamer

Setup and operation of power threading machine

Operation of power drills

Operation of torch

Safety meetings

	
	1.3K

	Installation of underground piping and accessories

Installation of cast iron pipe and fittings

Installation of plastic pipe and fittings

Installation of valves, post indicators, and hydrants

Rodding and thrust block installation

Valve pit installation

Flushing and testing of underground piping

Safety meetings

	
	400

	Wet pipe systems

Distribution of system

Installation of feed mains and cross mains

Branch line installation

Installation of hangers and system supports

Installation of valves including their trim

Installation of fire department connections

Setup and testing of system

Safety meetings

	
	1.6K

	Dry pipe systems

Distribution of system

Installation of feed mains and cross mains

Branch line installation

Installation of hangers and system supports

Installation of valves including their trim

Installation of fire department connections

Setup and testing of system

Safety meetings

	
	600

	Standpipe systems

Distribution of system

Pipe installation

Installation of hose, hose valve assemblies, nozzles, and accessories

System testing

Safety meetings

	
	500

	Special hazard systems

Installation of deluge systems

Installation of preaction systems

Installation of clean agent systems

Installation of carbon dioxide systems

Installation of fire extinguishers

Installation of nitrogen generators

Safety meetings

	
	400

	Fire pumps and accessories

Setting of fire pumps and jockey pumps

Alignment of fire pump and driver

Installing trim for fire pump and jockey pump

Installing fire pump controllers

Start up and testing of fire pumps and equipment

Safety meetings

	
	400

	Maintenance and repairs

Fabrication and installation of pipe on the job site

Care in cutting and patching of walls and ceilings

Repair and replacement of system components

Restoring system(s) to service

Notifying owner, fire department, and insurance company of impairment to system

Safety meetings

	
	600

	Totals
	
	OJT HRS
8K
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	Related Instruction Online
	RSI HRS

	Building Your Future in Construction
	2

	Basic Safety
	12

	Introduction to Construction Math
	10

	Introduction to Hand Tools
	12

	Introduction to Power Tools
	10

	Introduction to Construction Drawings
	10

	Basic Rigging
	7

	Basic Communication Skills
	7

	Basic Employability Skills
	7

	Introduction to Material Handling
	5

	Occupational Overview: The Sprinkler Industry
	5

	Introduction to Components & Systems
	10

	Steel Pipe and Fittings
	20

	CPVC Pipe and Fittings
	12

	Copper Tube and Fittings
	10

	Underground Pipe
	12

	Hangers, Supports, and Restraints
	17

	General Purpose Valves
	15

	Math for Sprinkler Fitters
	20

	Shop Drawings
	30

	Standard Spray Sprinklers
	20

	Wet Pipe Sprinkler Systems
	25

	Dry Pipe Sprinkler Systems
	25

	Deluge & Preaction Systems
	35

	Standpipes
	25

	Water Supplies
	15

	Fire Pump Systems
	35

	Application-Specific and Special Sprinklers
	40

	Totals
	RSI HRS
450




