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	Work Process Schedule
	
	OJT HRS

	Maintain safety.

Operate safety equipment and use safe work habits.

	
	100

	Measure dimensions of completed products or workpieces to verify conformance to specifications.

Examine workpieces for defects and measure workpieces with straightedges or templates to ensure conformance with specifications.

Check grooves, angles, or gap allowances, using micrometers, calipers, and precision measuring instruments.

	
	300

	Operate welding equipment.

Weld components in flat, vertical, or overhead positions.

Recognize, set up, and operate hand and power tools common to the welding trade, such as shielded metal arc and gas metal arc welding equipment.

Select and install torches, torch tips, filler rods, and flux, according to welding chart specifications or types and thicknesses of metals.

Weld separately or in combination, using aluminum, stainless steel, cast iron, and other alloys.

Ignite torches or start power supplies and strike arcs by touching electrodes to metals being welded, completing electrical circuits.

Guide and direct flames or electrodes on or across workpieces to straighten, bend, melt, or build up metal.

	
	900

	Notify others of equipment repair or maintenance needs.

Detect faulty operation of equipment or defective materials and notify supervisors.

	
	100

	Watch operating equipment to detect malfunctions.

Detect faulty operation of equipment or defective materials and notify supervisors.

	
	100

	Select production equipment according to product specifications.

Select and install torches, torch tips, filler rods, and flux, according to welding chart specifications or types and thicknesses of metals.

Determine required equipment and welding methods, applying knowledge of metallurgy, geometry, and welding techniques.

	
	250

	Clean workpieces or finished products.

Prepare all material surfaces to be welded, ensuring that there is no loose or thick scale, slag, rust, moisture, grease, or other foreign matter.

	
	100

	Determine metal or plastic production methods.

Determine required equipment and welding methods, applying knowledge of metallurgy, geometry, and welding techniques.

	
	100

	Mark products, workpieces, or equipment with identifying information.

Mark or tag material with proper job number, piece marks, and other identifying marks as required.

	
	100

	Align parts or workpieces to ensure proper assembly.

Align and clamp workpieces together, using rules, squares, or hand tools, or position items in fixtures, jigs, or vises.

	
	150

	Melt metal, plastic, or other materials to prepare for production.

Melt and apply solder along adjoining edges of workpieces to solder joints, using soldering irons, gas torches, or electric-ultrasonic equipment.

Melt and apply solder to fill holes, indentations, or seams of fabricated metal products, using soldering equipment.

	
	200

	Solder parts or workpieces.

Melt and apply solder along adjoining edges of workpieces to solder joints, using soldering irons, gas torches, or electric-ultrasonic equipment.

Melt and apply solder to fill holes, indentations, or seams of fabricated metal products, using soldering equipment.

	
	300

	Adjust equipment controls to regulate gas flow.

Connect and turn regulator valves to activate and adjust gas flow and pressure so that desired flames are obtained.

	
	100

	Monitor equipment operation to ensure that products are not flawed.

Monitor the fitting, burning, and welding processes to avoid overheating of parts or warping, shrinking, distortion, or expansion of material.

	
	300

	Mount materials or workpieces onto production equipment.

Position and secure workpieces, using hoists, cranes, wire, and banding machines or hand tools.

	
	300

	Operate grinding equipment.

Grind, cut, buff, or bend edges of workpieces to be joined to ensure snug fit, using power grinders and hand tools.

Chip or grind off excess weld, slag, or spatter, using hand scrapers or power chippers, portable grinders, or arc-cutting equipment.

Clean or degrease parts, using wire brushes, portable grinders, or chemical baths.

	
	600

	Reshape metal workpieces to established specifications.

Grind, cut, buff, or bend edges of workpieces to be joined to ensure snug fit, using power grinders and hand tools.

Repair products by dismantling, straightening, reshaping, and reassembling parts, using cutting torches, straightening presses, and hand tools.

	
	400

	Cut industrial materials in preparation for fabrication or processing.

Grind, cut, buff, or bend edges of workpieces to be joined to ensure snug fit, using power grinders and hand tools.

	
	100

	Ignite fuel to activate heating equipment.

Ignite torches or start power supplies and strike arcs by touching electrodes to metals being welded, completing electrical circuits.

	
	100

	Trim excess material from workpieces.

Chip or grind off excess weld, slag, or spatter, using hand scrapers or power chippers, portable grinders, or arc-cutting equipment.

	
	200

	Operate firefighting equipment.

Use fire suppression methods in industrial emergencies.

	
	100

	Design templates or patterns.

Develop templates and models for welding projects, using mathematical calculations based on blueprint information.

	
	100

	Disassemble equipment for maintenance or repair.

Repair products by dismantling, straightening, reshaping, and reassembling parts, using cutting torches, straightening presses, and hand tools.

	
	200

	Repair parts or assemblies.

Repair products by dismantling, straightening, reshaping, and reassembling parts, using cutting torches, straightening presses, and hand tools.

	
	100

	Heat material or workpieces to prepare for or complete production.

Preheat workpieces prior to welding or bending, using torches or heating furnaces.

	
	100

	Clean production equipment.

Clean or degrease parts, using wire brushes, portable grinders, or chemical baths.

	
	100

	Assemble temporary equipment or structures.

Set up and use ladders and scaffolding as necessary to complete work.

	
	100

	Shape metal workpieces with hammers or other small hand tools.

Hammer out bulges or bends in metal workpieces.

	
	100

	Operate metal or plastic forming equipment.

Operate metal shaping, straightening, and bending machines, such as brakes and shears.

	
	200

	Review blueprints or other instructions to determine operational methods or sequences.

Analyze engineering drawings, blueprints, specifications, sketches, work orders, and material safety data sheets to plan layout, assembly, and operations.

	
	100

	Totals
	
	OJT HRS
6K
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	Related Instruction Online
	RSI HRS

	Welding Engineering Technology/Technician
	300

	Welding Technology/Welder
	370

	Totals
	RSI HRS
670




