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	Work Process Schedule
	SKILLS
	OJT HRS

	Protect structures or surfaces near work areas to avoid damage.

Fill cracks, holes, or joints with caulk, putty, plaster, or other fillers, using caulking guns or putty knives.

Cover surfaces with dropcloths or masking tape and paper to protect surfaces during painting.

	2

	390

	Apply material to fill gaps in surfaces.

Smooth surfaces, using sandpaper, scrapers, brushes, steel wool, or sanding machines.

Read work orders or receive instructions from supervisors or homeowners to determine work requirements.

	2

	390

	Prepare surfaces for finishing.

Apply primers or sealers to prepare new surfaces, such as bare wood or metal, for finish coats.

Apply paint, stain, varnish, enamel, or other finishes to equipment, buildings, bridges, or other structures, using brushes, spray guns.

	2

	190

	Assemble temporary equipment or structures.

Erect scaffolding or swing gates, or set up ladders, to work above ground level.

	1

	390

	Mix substances or compounds needed for work activities.

Mix and match colors of paint, stain, or varnish with oil or thinning and drying additives to obtain desired colors and consistencies.

	1

	390

	Estimate construction project costs.

Calculate amounts of required materials and estimate costs, based on surface measurements or work orders.

	1

	390

	Tool applications and clean surfaces in preparation for work activities. Select construction equipment.

Select and purchase tools or finishes for surfaces to be covered, considering durability, ease of handling, methods of application, and customers' wishes.

Polish final coats to specified finishes.

	2

	390

	Substrate preparation and surface profile

Remove old finishes by stripping, sanding, wire brushing, burning, or using water or abrasive blasting.

	1

	390

	Protect structures or surfaces near work areas to avoid damage.

Remove fixtures such as pictures, door knobs, lamps, or electric switch covers prior to painting.

	1

	390

	Apply decorative or textured finishes or coverings.

Use special finishing techniques such as sponging, ragging, layering, or faux finishing.

	1

	390

	Apply decorative or textured finishes or coverings.

Cut stencils and brush or spray lettering or decorations on surfaces.

	1

	390

	Apply sealants or other protective coatings.

Waterproof buildings, using waterproofers or caulking.

Spray or brush hot plastics or pitch onto surfaces.

Bake finishes on painted or enameled articles, using baking ovens.

	3

	390

	Construction Safety

PPE use and fitment, PPE helmet NOVA 3, OSHA stand down program, abrasive blasting, fall protection, confined space, use of ladders, scaffolds, platforms.

Manlift operation and safety, bucket truck use and safety.

	2

	390

	Totals
	SKILLS
20
	OJT HRS
4K
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	Related Instruction Online
	RSI HRS

	Introduction to painter construction trade
	24

	Equipment and maintenance
	36

	Surface preparation and cleaning
	36

	Non-spray application of coatings-brushing, rolling and transfer
	36

	Construction materials coating applied substrates
	16

	Spray painting-airless, conventional, airless assisted
	48

	Wallcoverings-booking, trimming, application of
	12

	Abrasive blasting-dry, wet, dustless, abrasive blasting, PPE use
	36

	Wood finishing-stain, varnish, oiled, sealing, two components
	10

	Decorative finishing-faux, venetian, libero, stuhhi
	14

	Construction safety-OSHA, lift operation, fall protection, confined space, OSHA “stand down” classroom
	36

	Business fundamentals as applied to painting construction
	16

	Construction safety-use of equipment, ladders, scaffolding, ancillary safety, PPE fitment
	36

	Overspray awareness and prevention
	4

	Totals
	RSI HRS
360




