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	Work Process Schedule
	
	OJT HRS

	Install plumbing or piping.

Install underground storm, sanitary, or water piping systems, extending piping as needed to connect fixtures and plumbing.

Assemble pipe sections, tubing, or fittings, using couplings, clamps, screws, bolts, cement, plastic solvent, caulking, or soldering, brazing, or welding equipment.

Install pipe assemblies, fittings, valves, appliances such as dishwashers or water heaters, or fixtures such as sinks or toilets, using hand or power tools.

Anchor steel supports from ceiling joists to hold pipes in place.

Attach pipes to walls, structures, or fixtures, such as radiators or tanks, using brackets, clamps, tools, or welding equipment.

Install pipe systems to support alternative energy-fueled systems, such as geothermal heating or cooling systems.

	
	1.4K

	Maintain plumbing structures or fixtures.

Shut off steam, water, or other gases or liquids from pipe sections, using valve keys or wrenches.

Modify, clean, or maintain pipe systems, units, fittings, or related machines or equipment, using hand or power tools.

Maintain or repair plumbing by replacing defective washers, replacing or mending broken pipes, or opening clogged drains.

	
	710

	Weld metal components.

Assemble pipe sections, tubing, or fittings, using couplings, clamps, screws, bolts, cement, plastic solvent, caulking, or soldering, brazing, or welding equipment.

Attach pipes to walls, structures, or fixtures, such as radiators or tanks, using brackets, clamps, tools, or welding equipment.

Weld small pipes or special piping, using specialized techniques, equipment, or materials, such as computer-assisted welding or microchip fabrication.

	
	710

	Mark reference points on construction materials.

Locate and mark the position of pipe installations, connections, passage holes, or fixtures in structures, using measuring instruments such as rulers or levels.

	
	240

	Measure materials or objects for installation or assembly.

Locate and mark the position of pipe installations, connections, passage holes, or fixtures in structures, using measuring instruments such as rulers or levels.

	
	240

	Create construction or installation diagrams.

Lay out full scale drawings of pipe systems, supports, or related equipment, according to blueprints.

	
	240

	Cut metal components for installation.

Cut, thread, or hammer pipes to specifications, using tools such as saws, cutting torches, pipe threaders, or pipe benders.

	
	240

	Fabricate parts or components.

Cut, thread, or hammer pipes to specifications, using tools such as saws, cutting torches, pipe threaders, or pipe benders.

	
	240

	Plan layout of construction, installation, or repairs.

Plan pipe system layout, installation, or repair, according to specifications.

	
	240

	Inspect plumbing systems or fixtures.

Fill pipes or plumbing fixtures with water or air and observe pressure gauges to detect and locate leaks.

Inspect, examine, or test installed systems or pipe lines, using pressure gauge, hydrostatic testing, observation, or other methods.

	
	470

	Review blueprints or specifications to determine work requirements.

Review blueprints, building codes, or specifications to determine work details or procedures.

	
	240

	Select construction materials.

Select pipe sizes, types, or related materials, such as supports, hangers, or hydraulic cylinders, according to specifications.

	
	240

	Direct construction or extraction personnel.

Direct helpers engaged in pipe cutting, preassembly, or installation of plumbing systems or components.

	
	240

	Clean equipment or facilities.

Modify, clean, or maintain pipe systems, units, fittings, or related machines or equipment, using hand or power tools.

	
	240

	Estimate construction project costs.

Estimate time, material, or labor costs for use in project plans.

	
	240

	Estimate construction project labor requirements.

Estimate time, material, or labor costs for use in project plans.

	
	120

	Install gauges or controls.

Install automatic controls to regulate pipe systems.

	
	240

	Record operational or environmental data.

Keep records of work assignments.

	
	120

	Inspect work sites to determine condition or necessary repairs.

Inspect structures to assess material or equipment needs, to establish the sequence of pipe installations, or to plan installation around obstructions, such as electrical wiring.

	
	240

	Repair worn, damaged, or defective mechanical parts.

Repair or remove and replace system components.

Repair hydraulic or air pumps.

	
	470

	Remove parts or components from equipment.

Repair or remove and replace system components.

	
	240

	Replace worn, damaged, or defective mechanical parts.

Repair or remove and replace system components.

	
	120

	Cut openings in existing structures.

Cut openings in structures to accommodate pipes or pipe fittings, using hand or power tools.

	
	240

	Inspect work sites to identify potential environmental or safety hazards.

Inspect work sites for obstructions or holes that could cause structural weakness.

	
	120

	Install green plumbing or water handling systems.

Install green plumbing equipment, such as faucet flow restrictors, dual-flush or pressure-assisted flush toilets, or tankless hot water heaters.

Install fixtures, appliances, or equipment designed to reduce water or energy consumption.

	
	470

	Operate pumps or compressors.

Operate motorized pumps to remove water from flooded manholes, basements, or facility floors.

	
	240

	Totals
	
	OJT HRS
8.5K
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	Related Instruction Online
	RSI HRS
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	RSI HRS
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