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	Work Process Schedule
	
	OJT HRS

	Clean work sites.

Follow established safety rules and regulations and maintain a safe and clean environment.

	
	200

	Mark reference points on construction materials.

Measure and mark cutting lines on materials, using a ruler, pencil, chalk, and marking gauge.

	
	200

	Measure materials or objects for installation or assembly.

Measure and mark cutting lines on materials, using a ruler, pencil, chalk, and marking gauge.

	
	200

	Assemble temporary equipment or structures.

Erect scaffolding or ladders for assembling structures above ground level.

Assemble and fasten materials to make frameworks or props, using hand tools and wood screws, nails, dowel pins, or glue.

Construct forms or chutes for pouring concrete.

	
	600

	Cut wood components for installation.

Shape or cut materials to specified measurements, using hand tools, machines, or power saws.

	
	200

	Review blueprints or specifications to determine work requirements.

Study specifications in blueprints, sketches, or building plans to prepare project layout and determine dimensions and materials required.

	
	200

	Verify alignment of structures or equipment.

Verify trueness of structure, using plumb bob and level.

	
	200

	Build construction forms or molds.

Construct forms or chutes for pouring concrete.

	
	200

	Install carpet or flooring.

Cover subfloors with building paper to keep out moisture and lay hardwood, parquet, or wood-strip-block floors by nailing floors to subfloor or cementing them to mastic or asphalt base.

	
	200

	Install wooden structural components.

Install structures or fixtures, such as windows, frames, floorings, trim, or hardware, using carpenters' hand or power tools.

Build or repair cabinets, doors, frameworks, floors, or other wooden fixtures used in buildings, using woodworking machines, carpenter's hand tools, or power tools.

Examine structural timbers and supports to detect decay, and replace timbers as required, using hand tools, nuts, and bolts.

	
	600

	Coordinate construction project activities.

Arrange for subcontractors to deal with special areas, such as heating or electrical wiring work.

	
	200

	Inspect work sites to determine condition or necessary repairs.

Inspect ceiling or floor tile, wall coverings, siding, glass, or woodwork to detect broken or damaged structures.

Examine structural timbers and supports to detect decay, and replace timbers as required, using hand tools, nuts, and bolts.

	
	400

	Apply decorative or textured finishes or coverings.

Finish surfaces of woodwork or wallboard in houses or buildings, using paint, hand tools, or paneling.

	
	200

	Install building fixtures.

Install structures or fixtures, such as windows, frames, floorings, trim, or hardware, using carpenters' hand or power tools.

Install rough door and window frames, subflooring, fixtures, or temporary supports in structures undergoing construction or repair.

	
	400

	Install doors or windows.

Install structures or fixtures, such as windows, frames, floorings, trim, or hardware, using carpenters' hand or power tools.

Install rough door and window frames, subflooring, fixtures, or temporary supports in structures undergoing construction or repair.

	
	400

	Prepare operational reports.

Maintain records, document actions, and present written progress reports.

	
	200

	Remove worn, damaged or outdated materials from work areas.

Remove damaged or defective parts or sections of structures and repair or replace, using hand tools.

	
	200

	Order construction or extraction materials or equipment.

Select and order lumber or other required materials.

	
	200

	Select construction materials.

Select and order lumber or other required materials.

	
	200

	Prepare hazardous waste for processing or disposal.

Work with or remove hazardous material.

	
	200

	Record operational or environmental data.

Maintain job records and schedule work crew.

	
	200

	Apply material to fill gaps in surfaces.

Fill cracks or other defects in plaster or plasterboard and sand patch, using patching plaster, trowel, and sanding tool.

	
	200

	Position construction forms or molds.

Anchor and brace forms and other structures in place, using nails, bolts, anchor rods, steel cables, planks, wedges, and timbers.

	
	200

	Estimate construction project costs.

Prepare cost estimates for clients or employers.

	
	200

	Drill holes in construction materials.

Bore boltholes in timber, masonry or concrete walls, using power drill.

	
	200

	Install safety or support equipment.

Install rough door and window frames, subflooring, fixtures, or temporary supports in structures undergoing construction or repair.

	
	200

	Mix substances or compounds needed for work activities.

Perform minor plumbing, welding, or concrete mixing work.

	
	200

	Weld metal components.

Perform minor plumbing, welding, or concrete mixing work.

	
	200

	Dig holes or trenches.

Dig or direct digging of post holes and set poles to support structures.

	
	200

	Direct construction or extraction personnel.

Dig or direct digging of post holes and set poles to support structures.

	
	200

	Position safety or support equipment.

Dig or direct digging of post holes and set poles to support structures.

	
	200

	Install trim or paneling.

Apply shock-absorbing, sound-deadening, or decorative paneling to ceilings or walls.

	
	200

	Assemble products or production equipment.

Build sleds from logs and timbers for use in hauling camp buildings and machinery through wooded areas.

	
	200

	Totals
	
	OJT HRS
8K
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	Related Instruction Online
	RSI HRS

	Safety and Worksite Management
	12

	Measurement and Layout
	16

	Construction Materials and Methods
	16

	Structural Assembly
	20

	Installation Techniques
	20

	Inspection and Quality Control
	16

	Specialized Skills
	16

	Project Management and Documentation
	16

	Totals
	RSI HRS
130




