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	Work Process Schedule
	
	OJT HRS

	Poles, Arms, and guys

Dig pole holes in ordinary soil, rock, hard pan, swamp

Locate poles with proper regard to property lines, sidewalks, ditches, etc.

Load and unload poles on trailers, trucks, or cars

Roof and frame poles

Set poles with derrick and with pikes

Face, straighten and line in poles

Place 'heel and toe' on self-supporting poles

Fill and tamp around pole

Stub a decayed pole

Move a pole by trenching

Test poles for decay, using test bar

Replace poles by digging new hole beside old pole

Replace poles by pulling old butt and reaming hole

Select proper arm for job

Install single arm and buck arm

Install double arm with space bolts

Install alley arm

Install pins and deadend bolts in arm

Make up guy wire body and tails using clamps and also by serving wire

Install all types of anchors-legs, expanding cone, swamp, etc.

Install all types of guy-sidewalk, span, arm, anchor, etc.

Methods of proper rigging.

	
	1.6K

	Conductors, switches, protective devices

Stringing of conductors

Bare copper and aluminum, W.P. copper and aluminum

Splicing conductors, copper and aluminum

Dying in conductors, copper and aluminum

Making conductor to conductor taps, copper and aluminum and combinations of both

Install common types of insulators

Trimming trees to clear wires

Remove conductors being replaced

Install single pole disconnecting switches

Install gang-operated switches

Install line fuses

Install pole-mounted oil switches

Install capacitor banks

Install lightning arrestors

Install and operate line reclosers

Install and operate line sectionalizing apparatus

	
	1.7K

	Transformers

Install cutouts and proper fuses

Install and connect a single-phase transformer for 120-volt two-wire load and 120/240-volt three-wire load

Install and connect an additional transformer to secondary bus fed by other transformers

Install and connect three transformers-wye-delta

Install and connect two transformers-wye-delta

Connect transformer bank to supply 240-volt three-phase and 120/240-volt single-phase service

Connect transformer bank to supply combination 208-volt three-phase and 120/208-volt single-phase service

Connect additional transformers to feed a three-phase bus feed from another source

Relation and phasing

Use of instruction, voltmeters, ammeters, phase sequence indicators, etc.

Connect current and potential transformers for metering

Install and operate voltage regulating apparatus

	
	900

	Underground work experience

Circuitry of underground equipment

System maps and circuit diagrams

Underground job layout

Subsurface structures and trenches

Cable and equipment installation

Operations and maintenance of underground system

Service drops and meters

Safety

Substation Orientation

Miscellaneous

	
	

	Totals
	
	OJT HRS
4.1K
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	Related Instruction Online
	RSI HRS

	Supervised field trips
	

	Sponsor approved training seminars

Requests for training seminars must be submitted in writing to the committee 30 days prior to the scheduled date of the training seminars. Training Seminars must be preapproved by the committee.
	

	Sponsor approved online or distance learning courses

Requests for online or distance learning courses must be submitted in writing to the committee 30 days prior to the scheduled date of the online or distance learning courses. Online or distance learning courses must be preapproved by the committee.
	

	State Community/Technical college

Seattle Community College
	

	Other

Camp Rilea, Northwest Line Constructors Apprenticeship Electrical Course; and any other training or facilities as approved by the Committee.
	

	Totals
	RSI HRS
0




