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	Work Process Schedule
	SKILLS
	OJT HRS

	Operate pumps or compressors
Tend pumps, compressors, or generators to provide power for tools, machinery, or equipment or move materials.

	0

	180

	Clean equipment or facilities
Lubricate, clean, or repair machinery, equipment, or tools.

	0

	130

	Lockout Tagout

	0

	70

	Maintain construction tools or equipment
Lubricate, clean, or repair machinery, equipment, or tools.

	0

	180

	Signal equipment operators to indicate proper equipment positioning
Signal equipment operators to facilitate alignment, movement, or adjustment of machinery, equipment, or materials.

	0

	300

	Install green structural components, equipment or systems

	0

	130

	Direct vehicle traffic
Control traffic passing near, in, or around work zones.

	0

	200

	Review blueprints or specifications to determine work requirements
Read plans, instructions, or specifications to determine work activities.

	0

	130

	Finish concrete surfaces
Smooth or finish freshly poured cement or concrete, using floats, trowels, screeds, or powered cement finishing tools.

	0

	60

	Test air quality at work sites
Operate or maintain air monitoring or other sampling devices in confined or hazardous environments.

	0

	12

	Clean work sites
Clean or prepare construction sites to eliminate possible hazards.

	0

	130

	Compact materials to create level bases
Dig ditches or trenches, backfill excavations, or compact and level earth to grade specifications, using picks, shovels, pneumatic tampers, or rakes.

	0

	50

	Dig holes or trenches
Dig ditches or trenches, backfill excavations, or compact and level earth to grade specifications, using picks, shovels, pneumatic tampers, or rakes.

	0

	90

	Mark reference points on construction materials
Measure, mark, or record openings or distances to layout areas where construction work will be performed.

	0

	60

	Measure work site dimensions
Measure, mark, or record openings or distances to layout areas where construction work will be performed.

	0

	60

	Assemble temporary equipment or structures
Erect or dismantle scaffolding, shoring, braces, traffic barricades, ramps, or other temporary structures.

	0

	60

	Dismantle equipment or temporary structures
Erect or dismantle scaffolding, shoring, braces, traffic barricades, ramps, or other temporary structures.

	0

	60

	Load or unload materials used in construction or extraction
Load, unload, or identify building materials, machinery, or tools, distributing them to the appropriate locations, according to project plans or specifications.

	0

	250

	Move construction or extraction materials to locations where they are needed
Load, unload, or identify building materials, machinery, or tools, distributing them to the appropriate locations, according to project plans or specifications.

	0

	250

	Assist skilled construction or extraction personnel
Provide assistance to craft workers, such as carpenters, plasterers, or masons.

	0

	250

	Apply paint to surfaces
Spray materials, such as water, sand, steam, vinyl, paint, or stucco, through hoses to clean, coat, or seal surfaces.

	0

	130

	Apply sealants or other protective coatings
Spray materials, such as water, sand, steam, vinyl, paint, or stucco, through hoses to clean, coat, or seal surfaces.

	0

	130

	Clean surfaces in preparation for work activities
Spray materials, such as water, sand, steam, vinyl, paint, or stucco, through hoses to clean, coat, or seal surfaces.

	0

	130

	Remove worn, damaged or outdated materials from work areas
Raze buildings or salvage useful materials.

	0

	130

	Position construction forms or molds
Position or dismantle forms for pouring concrete, using saws, hammers, nails, or bolts.

	0

	90

	Smooth surfaces with abrasive materials or tools
Grind, scrape, sand, or polish surfaces, such as concrete, marble, terrazzo, or wood flooring, using abrasive tools or machines.

	0

	90

	Install masonry materials
Place, consolidate, or protect case-in-place concrete or masonry structures.

	0

	90

	Protect structures or surfaces near work areas to avoid damage
Place, consolidate, or protect case-in-place concrete or masonry structures.

	0

	90

	Mix substances or compounds needed for work activities
Mix ingredients to create compounds for covering or cleaning surfaces.

	0

	90

	Break up rock, asphalt, or concrete
Operate jackhammers or drills to break up concrete or pavement.

	0

	60

	Pour materials into or on designated areas
Mix, pour, or spread concrete, using portable cement mixers.

	0

	90

	Prepare hazardous waste for processing or disposal
Identify, pack, or transport hazardous or radioactive materials.

	0

	180

	Utilize GPS lasers for elevation issues
Setup tooling to level materials.

	0

	130

	Grade control

	0

	250

	Totals
	SKILLS
0
	OJT HRS
4.3K
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